|  |  |
| --- | --- |
| Model | SP20,000™ (Integrated Controls) |
| Part Number | ITD4700 |
| Boom Rating | 20,000 lb. |
| Winch Rating | 20,000 lb. |
| Wire Rope Size | 9/16" x 150 |
|  Free Spool | Air Operated |
| Tie Back Anchor Points | 8 ( Removable-D-Ring (2) Std ) |
| Wireless Remote Control For all Hyd Functions  | Yes |
| All Hydraulic Functions Pre Plumbed to SP Valve Body | Yes |
| Requires Additional Hydraulic Valving / Controls | No |
| Self-Leveling Pavement Pads | Yes |
| Fold Down Ground Penetrating Grousers | Yes |
| Light Bar Mounting Base | Optional |
| Polished Stainless Steel Rear Panel | Not Available |
| Removable Outer Recovery Boom Head | Yes |
| Center Boom Head Can be Used For Recoveries | Yes |
| Available Tuff Coat Black, Yellow or Primer Gray | Yes |
| Min Recommended Chassis Height | 40" |
| Max Recommended Chassis Height | 46" |
| Minimum Recommended Chassis GVWR | 30,000 lb. |
| Maximum Recommended Chassis GVWR | 55,000 lb. |
| Shipping Weight | 2,200 lb. |