CONDOR® E-TRACK-ADAPTOR-R INSTRUCTION MANUAL

STOP! WARNING:  READ THIS FIRST!
First read and understand the instruction manual and product labels for important safety, set-up and troubleshooting information.  If you have problems setting up or using the CONDOR® E-TRACK-ADAPTOR-R, contact customer service at (815) 754-7418 or contact us via email @ www.condor-lift.com.  The CONDOR® E-TRACK-ADAPTOR-R is not intended for use by children.

Assembly Instructions: Remove all parts from shipping box. Check the parts below to make sure you have all the parts needed to assemble your CONDOR® TRACK-ADAPTOR-R, before beginning.  In the unlikely event that you find a part damaged or missing, please call customer service @ 815-754-7418. 

	Component Photo
	Item
	Component Description
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	A
	Main Adaptor Base
	1
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	B
	Leveling Pad w/ Adjustment Nut
	4
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	C
	E-Track HD Clip
	2

	
[image: image4.png]



	D
	½” x ¾” x 3/8”-16 Shoulder Bolt
	2
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	E
	5/16”-18 x ½” Button Head
	6


                         You will need the following tools for assembly: (1) 6mm Hex Key (Included)
ASSEMBLY:

1. Attach each E-Track HD Clip to either side facing opposite directions using the Shoulder bolts. The clip lock should be offset in the same direction as tapped hole so the unit remains centered on the track. (see below)  
2. Attach all 4 Leveling Pads from underneath the unit and roughly adjust for height, depending on depth and placement of the E-track itself. 
3. Place the unit onto the E-Track and engage both clips to secure.  If fit is too tight, loosen the shoulder bolts to attach, and then re-tighten the shoulder bolts.
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USER INSTRUCTIONS:

1. Using the 4 Button Head Screws provided, attach the chock to the adaptor in either the Parallel or Perpendicular direction.  Secure vehicle in the desired orientation with appropriate tie downs.
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CAUTION: 

Always make sure that all fasteners are tight and all pins are in place prior to use.  Understand the limitations of this product and do not exceed these limitations. Always make sure that the wheel chock’s cradle setting is optimum for the tire size of the motorcycle before use.  Be sure to read and understand user instructions for the CONDOR® E-TRACK-ADAPTOR-R If instructions are not clear, additional information is available at www.condor-lift.com or call (800) 461-1344.  Technical Components Development & Design is not responsible for any damage incurred by exceeding this product’s limitations in structure and/or functionality.

One Year Limited Warranty:

This CONDOR® E-TRACK-ADAPTOR-R product warranty extends to the original consumer purchaser of the product.  All illustrations and specifications contained in this manual are based on the latest product information available at the time of printing.  Technical Components Development & Design, Inc. reserves the right to make changes at any time, without notice, in color, material, equipment, options, specifications and models.  Models may be shown with optimal equipment.  Further information may be obtained by contacting Technical Components Development & Design, Inc. at (815) 754-7418.

Return Policy:
15 day return policy applies.  Merchandise may be returned within 15 days of purchase.  Merchandise must be unused and in its original packaging.  Customer will call TC Development for a Return Authorization number. Customer pays for freight return.  Credit is given upon inspection of returned goods.  A 15% re-stocking fee applies to all returned merchandise.  If the product was originally shipped with a free shipping promotion, the cost of shipping will be deducted from the dollar amount of the return in addition to the restocking fee.
Warranty Duration:
This product is warranted to the original consumer purchase for a period of one (1) year from the original purchase date. 

What is not covered:
Our warranty will not cover abnormal wear of parts, damage resulting from negligent use of misuse of the product, use contrary to operating instructions, or disassembly, repair or alteration by any person other than an authorized service station.  We shall not be liable for any incidental of consequential damages for breach of by express or implied warranty on products.

How your state’s law may apply:
Some states do not allow limitations on how long any implied warranty lasts or the exclusion or limitation or incidental or consequential damages, so the above limitations may not apply to you.  This warranty gives you specific rights, and you may also have other rights, which may vary from state to state.

Thank you for purchasing the CONDOR® E-TRACK-ADAPTOR-R.
CONDOR® is a trademark of Technical Components Development & Design, Inc.

210 Stephenie Dr.

Cortland, IL 60112

Phone: (815) 754-7418

Fax: (815) 754-7419

Website: www.condor-lift.com
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